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Serving Monterey, San Benito, and Santa Cruz Counties
24580 Silver Cloud Court


Monterey, CA  93940




PHONE: (831) 647-9411 • FAX: (831) 647-8501

GENERAL APPLICATION – FLEET ORVR EXEMPTION FORM

For claiming exemption from Phase II requirements per Rule 1002 Section 1.3.4

	Company Name:
	MBARD Permit Number (Existing Facilities Only)

	DBA:

	Equipment Description:

	Equipment Location: 

	1. Does your GDF refuel vehicles that are owned by a common operator?
· Yes ( Go to Part 2)
· No (STOP. You do not qualify for this exemption)

	2. What is the total number of vehicles in the fleet?
	A = 

	3. What is the total number of ORVR Vehicles in Fleet
· Please fill out the information in Table A below. 

· Use Table B to help determine whether vehicles have ORVR.

· Each vehicle with a model year in the transition period must be verified. 
	B =

	4. Check for 90% of Fleet with ORVR

· Divide by B by A ( i.e. B /A) 

· If C is less than 0.90, STOP. You do not qualify for this exemption
	C=

	5. Certification/Signature of person responsible for the information on this form.
I hereby certify that I am authorized to complete this form for the facility and that all information contained herein is true and correct.

	Name:
	Title:



	Signature:


	Date
	Phone:


	Table A. List of Fleet Vehicles

	Agency Vehicle ID
	Class1
	Vehicle Make
	Vehicle Model
	Model Year
	VIN or S/N
	Evaporative Family 2
	Is Vehicle ORVR?3

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	


1. Class = Passenger Cars (PC), Light Duty Trucks (LDT), Light Duty Trucks/Medium Duty Vehicles (LDT/MDT)
2. The Evaporative Family code can be found within the engine compartment. The Evaporative Family code contains twelve (12) alpha-numerical characters. This code must be included for transition models.

3. See Table B below on “How to Determine ORVR.”

	Table B. How to determine if a gasoline-powered vehicle has onboard refueling vapor recovery (ORVR)

	1. Look for the emission label (tune-up label) in the engine compartment. It shows the model year and vehicle class. Always use the vehicle class printed on the emission label to determine the correct ORVR category.

2. For vehicles classified as Light Duty Trucks and Medium Duty Vehicles according to the emission label, also check the vehicle GVWR (Gross Vehicle Weight Rating) inside the driver’s door frame.

3. If the model falls within a transition range according to the table below, check the emission label again for the evaporative family code (this code must be included in Table A above for transition models).

• If the 5th character in the code is an “R”, the vehicle is ORVR compliant.

• If it is anything else, the vehicle is not ORVR compliant.


	VEHICLE CLASS
	WEIGHT CLASS
	NON-ORVR MODELS
	TRANSISITON MODELS
	ALWAYS ORVR MODELS

	Passenger Cars (PC)/Light Duty Vehicles (LDV)
	All
	Model year 1997 or older
	Model years 1998-1999
	Model year 2000 or newer

	Light Duty Trucks (LDT) / Medium-Duty Vehicles (MDV)
	GVWR 6,000 lbs. or less
	Model year 2000 or older
	Model year 2001-2002
	Model year 2003 or newer

	
	GVWR 6,000-8,500 lbs.
	Model year 2003 or older
	Model years 2004-2005
	Model year 2006 or newer

	
	GVWR 8,500 lbs. – 10,000 lbs.
	Model year 2003 or older
	Model years 2004 or newer
	None

	
	GVWR 10,000 lbs. or greater
	All
	None
	None


Example of Engine Label Showing Evaporative Code – The label will be located within the engine compartment, typical locations include under the hood, radiator shroud, or strut tower:
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